# Simple FM transmitter

Many times we want to make fm transmitter which is simple to build and has a good range. So here is a simple fm transmitter circuit which contains only few components and also has long range. C3 is a 1 - 40 pf trimmer capacitor and L1 is 8 to 10 turns of hookup wire of 22 guage
wound on 6mm form. The size of a standard pencil is also 6mm so you can use a round pencil as form to wind the coil. The optional resistor shown in figure 2 is to limit the voice sensitivity for example a 10K resistor will resist the voice signal coming from microphone more as compare to the 1K resistor. If you want sensitive microphone do not use optional resistor. For Antenna use a piece of 12 inch hookup wire. Set a blank spot on a fm radio and slightly adjust the trimmer capacitor with any non conductive tool to tune the transmitter.
Categories
Electronics Beginner Guide Tutorials
Blog
Audio Circuits
Power Supply Circuits
LED & Light Circuits
Battery Chargers
Radio & RF Circuits
Telephone Circuits
Test & Measurement
FM Transmitter Circuits
Store
Related Circuits
Best FM Transmitter
1.5V Wireless FM transmitter Circuit
FM TX
Stable FM Transmitter
Stable FM Transmitter Using LM2936 Regulator
Solar FM Tranmitter
Bird Microphone Transmitter
Long Range Stable FM Transmitter
High Power FM Transmitter
FM Tracking Transmitter
Transistor FM Tracking Transmitter
Circuit Diagram
About
Contact
Links
Home
Sponsored Links
Privacy Policy
Copyright 2014 © CircuitDiagram.Org. All rights reserved.
Hello Readers, We frequently add new circuit diagrams, so do not forget to come back often. Thank you.