Skip to content
Sale!

# 6ES7 901-3DB30-0XA0

Rated 4.75 out of 5 based on 4 customer ratings
(4 customer reviews)

$72.00 – $99.00

Amsamotion Cable 4th generation 3DB30 Gold plated USB interface is the same as siemens USB PPI multi-master cable, be used for S7200 full range of Siemens S7-200 PLC and S7 touch screen programming download. Support PPI multi-master communication, the highest baud rate can reach 187.5k.

Model | Clear

6ES7 901-3DB30-0XA0 quantity
SKU: 32835159828 Category: SIEMENS PLC Cable Tags: 6es7 901 3db30 0xa0 driver, 6ES7 901-3DB30-0XA0, 6es7901-3db30-0xa0 price, amsamotion 3db30, usb/ppi multi-master cable 6es7 901-3db30-0xa0

- Description
- Additional information
- Reviews (4)

## Description

## 6Es7 901 3Db30 0Xa0 USB PPI Multi-Master Cable

Materials: Insulated and Environmental Protection PVC
Producing: China
Working Temperature:-30~70
Plug: Gold Plated
length:4.7m

Support Siemens HMI type:KTP600DP, KTP1000DP，TP177 micro, TP177A, TP 178,OP73, OP77A, Smart700/1000….

The Amsamotion Cable 4th generation 3DB30 with gold-plated USB interface is a device that allows you to connect a computer to a Siemens S7-200 PLC (Programmable Logic Controller) or S7 touch screen for programming and download purposes. It is similar to the Siemens USB PPI multi-master cable and is compatible with the full range of Siemens S7-200 PLCs. The cable has a USB connector on one end and a connector that is specific to the PLC or touch screen on the other end. It supports PPI multi-master communication and has a maximum baud rate of 187.5k. It is used in conjunction with software on the computer to communicate with the PLC or touch screen and transfer programming and configuration information.

Model | 3DB30+ | 901-3DB30
Chip | Ordinary chip | High-performance chip
Isolated | V | V
Gold plated interface | V | V
Connector | Straight 9 pins | Elbow 9 pins
Drive-free | V | V
Baud rate | 187.5Kbps | 187.5Kbps
Online monitoring | V | V

Video Player
00:00
00:00
00:00
Use Up/Down Arrow keys to increase or decrease volume.
1. 3db30
0:39

- Support S7-200 full series of PLC communication
- Support PPI multi master communication
- The highest baud rate reached 187.5kb
- Driver: no need to install driver, can be generated USB directly.
- System:Support Win7 (32/64bit)
- Full set: Packaging box+ Adapter (Include cable)

The amsamotion 3db30 don’t need install driver

Note

Siemens 6ES7901-3DB30-0XA0:SIMATIC S7, PC ADAPTER USB F. CONNECTION OF S7-200/300/ 400, C7; WITH USB-CABLE (5M) CAN BE USED UNDER WINXP/VISTA/ WINDOWS 7 32/64BIT

## Additional information

Weight | 0.45 kg
Brand | AMSAMOTION
Model | 3DB30+, 901-3DB30
Type | Gold plated Version

## 4 reviews for 6ES7 901-3DB30-0XA0

1. Rated 5 out of 5

   B***a – March 25, 2021

   Everithing ok! Reliable!

2. Rated 5 out of 5

   G***y – October 15, 2021

   Very. Very. Very fast. Received in less than 10 days It works perfect

3. Rated 5 out of 5

   R***v – January 12, 2022

   Super day came in very fast

4. Rated 4 out of 5

   Dennys Tucunango – May 30, 2023

   Please do you have a driver for run in Windows 10

Add a review Cancel reply
Your rating *

1 2 3 4 5

Your review *

Name *

Email *

Save my name, email, and website in this browser for the next time I comment.

Δ

## Related products

- Sale!

  ## PC-PPI

  $15.00 – $26.00 Select options
- Sale!

  ## 9AK1012-1AA00

  $59.00 $55.00 Add to cart
- Sale!

  ## 7MH4 702-8CA

  $81.00 $55.00 Add to cart
- Sale!

  ## 6ES7972-0CA23-0XA0

  $108.00 $72.00 Add to cart

Worldwide Free Shipping is guaranteed to global online consumers in AMSAMOTION.STORE. We guarantee total shopping satisfaction by offering exchange, Return or Refund Policy.